This archive contains the firmware for the Electronic Leadscrew by Rocketronics.de
Every hardware revision has its own folder.

Differences of the hardware versions:


Revision 3 has 6 keys in the lower row
Revision 4.0 has 7 black keys in the lower row
Revision 4.1 has 1 red key and 6 black keys in the lower row
Revision 5 has 8 keys in the lower row


Please select the correct folder and copy the contained files to your harddisk or a USB-Drive.
Then start the firmware update software "avrootloader.exe" and follow the instructions in the manual.

#################################################################################

Dieses Archiv enthält Firmware für die Elektronische Leitspindelsteuerung.

Für jede Hardware-Revision gibt es einen eigenen Ordner.


Unterschiede der Revisionen:

Revision 3   hat in der unteren Reihe 6 Tasten
Revision 4.0 hat in der unteren Reihe 7 schwarzeTasten
Revision 4.1 hat in der unteren Reihe 1 rote Taste und 6 schwarze Tasten
Revision 5   hat in der unteren Reihe 8 Tasten


Bitte wählen Sie den passenden Ordner und kopieren Sie die enthalteten Dateien in einen Ordner auf Ihre Festplatte oder einen USB-Stick.
Die genaue Vorgehensweise finden Sie unter

https://www.rocketronics.de/softwareaenderungen

