
363  26.10.2018

- New parameter submenu in many modes. The Submenu allows for easy change of common cutting parameters like
  Light feed, Tool corner radius etc.
  It is accessible by pressing FN + DOWN
  Exit is by pressing FN, or by navigating higher than the first entry.
  All settings visible there are also available in the normal system settings.

- A slower light feed is now available in the parameter menu, it is possible to set a percentage of the normal
  feed speed or a discrete speed in mm/U. This allowes for fast roughing and slow finishing

- New Drilling mode! With a drill in the tollholder you can now drill exact holes too.
  The new parameter submenu allows for selecting how to retract, total retraction or chip break.
  Depth of cut, chip break retracts and dwell time is also available as setting.

- New mode GROOVE: You can cut a circular groove with a setable depth.
  Important: Only possible with round cutters! Always set the cutter radius in the submenu.
  
- There are now 4 threading strategies available, the submenu in the thread modes allows for changing the parameters:
   - Radial infeed
   - Alternate flank
   - Flank infeed
   - Modified flank infeed
   Until this version the radial infeed was the only way, which resultes in heavy loads on small machines.
   We recommend using the flank infeed, which cuts only on the left flank of the cutter.
   To do this right it is need to set the thread angle correctly in the submenu! Metric threads have 60°,
   imperial 55°

- An error could lead to a creash when the spindel was on directly after startup, this is fixed.
- An error in angle mode messed up the display, this is also fixed.



362  03.10.2018

In the inner-cutting modes like Boring, Internal thread etc. it is now also possible to drive the x-axis to a position. The x axis stops at zero and at the position entered für XP, just like in all other modes.


360  10.06.2018

- Saving of the Feed-Settings is changed to limit the number of write cycles.
- The positions of X and Z is now saved for every mode until power down of the unit. Now the ELS shows positions for every mode, so you can easily switch from mode to mode without the need of reentering the desired positions.


359 12.02.2018
- The P0 key now sets the current position in ZP or XP when pressed if ZP or XP=0.
  So instead of setting XP or ZP to zero, if it is already zero you can update ZP or XP with the current position. This is handy when you want the current position be an endpoint for the next operation.
- For taper and radii the els now keeps a clearance in Z of at least 0.2mm.


358 Beta 11.01.2017
- First english software version
- Language can be selected in the settings menu


357 Beta 01.01.2018
- New mode UNDERCUT. This mode creates a thread undercut according to DIN EN 76-1
  The depth in X is all you need to enter, the lenth in Z is calculated by the control.
  It cuts a 30° taper, followed by a short straight way and ends in a defined radius
  ATTENTION: Only use 55° or 35° cutters, as others will cause a collision

